**JINXI Brand wide flange  steel beam price list and theoretical weight A36 grade**





|  |  |
| --- | --- |
| Grade | Q235,Q345,SS400,SS490,S235/S275,A36,A992,A572gr50 |
| H\*B | 100\*100-900\*300mm |
| T1 | 4.5-21mm |
| T2 | 7-35mm |
| Technique | Hot Rolled |
| Application | Mechanical&manufacture,Steel structure,Shipbuilding,Bridging, Automobile chassis  |
| MOQ | 20 Metric Ton/Metric Tons |
| Packaging Details | Bundled with firm steel straps, easy for loading |
| Delivery Time | 20 days after deposit |
| Payment Terms | L/C , T/T or Western Union |
| Supply Ability | 50000 Metric Ton/Metric Tons per Month |



















